I’ve rewritten the GPS driver to use ROS and a dynamically allocated buffer, which you can find in my “gpsdriver” archive.

The Seek LIDAR driver has not been rewrittten in this way, but I recommend it.